This gearbox has been built multiple times and has made prolonged runs in heavy Gauge 2 locos. It's intended for Nylon SLS but has been printed in filament printers. There are no supports. Requires 1/8" shafts and R144ZZ ball besring to complete. Note motor nose hole can be opened out for 540 series motor if you need 1/4 HP!