If using Slaters wheels, clear the axle holes in the axleboxes with a 4.8mm drill (should be possible with the drill bit held in fingers.) Push the Slaters bearing in almost all the way but with 1mm protruding. 