This is the 42mm Back to Back, G1MRA "Finescale" version - as per the "Coarsescale", a bearing substitute is included, that can be replaced if required with a 1/8" ID x 1/4" OD x 5/32" Wide ball bearing.