The handrails are rather vulnerable.  They are best made using some flexible, resilient material and due to their fine detail are perhaps best made on a resin printer.  Side of the body has holes to assist in positioning.  You will require two of each 'hand'.  I suggest you print some spares as well.