Two off.  These are preferably made from resilient material to withstand handling.  These are glued beneath the solebar, equally between the W-irons.  For increased stability they can also be tacked beneath the axle boxes.