Cab roof for the NSR battery-electric loco.  After painting the cab, insert the glazing.  The door windows need to be inserted from below, all the others from the top.  The cab can then be glued to the battery covers and the roof glued on top of the cab.  The roof, cab and battery covers make a complete assembly that should clip onto the body.