Four off.  These are the short version for springing.  Tap the hole M2 x 0.4.  Fit a spring from Peter Korzelius over an M2 screw, insert through the buffer housing into the threaded hole and tighten to leave about 3mm - 4mm movement.  Glue onto the buffer beam so the screw can move freely through the hole.