You will need a length of 3mm/1/8"  silver steel rod for the axle.  To retain the back to back dimension it is recommended that a 40mm length of brass tube is slid on the axle, between the wheels before they are pushed on to the axle.  Wheels can be painted before fitting to the axles.