These are mounted at each end of the brake activation rod.  When mounted on the rod, glue them to the solebar, with a small amount of rod emerging for the brake lever.  Fit the brake cylinder lever before gluing the rod in place.  