The W-irons and bolsters should be free to move from the springs.  One bolster assembly is fixed in position with two rods in the outer lateral holes in bolster and crossbeams.  The other bolster is allowed to pivot on a single rod inserted through the central holes.