Glue the brake gear into the corner between the solebar and the medial cross-beams.  Note the brake shoes should be inbound.  These early vehicles only had one pair of brake shoes working on a single axle.   You will also require a suitable length of 1mm silver steel rod to fit beneath the solebars and allow for mounting of the brake lever.