This 1st class coach body assembly is the second of three styles that use the common underframe uploaded 27/05/2025.
Glazing slots are provided for fitting glazing film (typically 0.25mm laminating pouches).
The coach roof is held to the body by printed retainers holding captive m3 nuts and countersunk screws.
An isometric assembly drawing and item list is provided.
The body assemblies are fastened to the underframe with 6 M3x16 countersunk screws.