In response to Keith's invitation to add a modified roof, here it is. This roof replaces the hollow rectangular under frames with a solid block extending 1mm lower. This may be easier to print for those having problems with the original thin roof. Note: if using this roof reduce the height of the "inner wall" by 5mm with a straight horizontal at the top.