Has the RCH end door body with the end door as a separate STL. Ideal for printing in resin to avoid pressure differential problems from having a sealed body. Print body upside down and door right way up (hinges at top). You may need to incorporate a few squares to help with adhesion to the build plate, and 1 small support for each door locking ring which projects from the side.