I printed face up, 100% infill and with support at 10% density. Slaters wheel will run in the centre with vertical movement (no bearing). Other (non-pivoting) axle runs in a standard slaters bearing. 