Print on its end if you can with a brim. I used 0.2mm layer height, 20% infill and support at 20% density. 

On the underside is a cut out to take dolls-house style LED lighting eg https://www.amazon.co.uk/gp/product/9302259897/ (cut in half at the mark) and a 9v battery