This is held in place by a 1/16" piece of stainless rod that runs the length of the wagon and is fixed to the coupling hooks at each end. After printing this piece it helps to run a 1.6mm bit through the hole a few times so that it pivots freely. Slaters wheel bearings should be a tight push fit in the two large holes. 