The side has a cutout on the reverse that helps alignment of this end piece. The pipe that runs along the top overlaps the side piece and will need cleaning up after printing to ensure it isn't interfering with the fit.  

Two holes are provided to locate the two hoses at each end of the van. The hoses from the BR Cattle Wagon posted here could be used (with the bottom locator cut off)