One piece body with modified window arrangement. Have printed successfully at 0.12mm layer height. Produces a strong and square body. Will likely need heated bed, a brim and some sort of plate adhesive (e.g. magigoo) to stop the corners lifting when printing. 