Single piece body. Ideally print with 0.12 or 0.16 layer height. Will need a decent brim to hold it to the print bed (otherwise will lift in corners) and may need support (I used 8% support touching the printbed only and no-where else)